

**How to upgrade the firmware ?**


Step1, Switch flatbed cutter on, then connect flatbed cutter to computer through USB cable

Step2, To run enclosed "FirmWare.exe"





Step3, To choose enclosed"Flatbed-1.00.03.bin"



Step4, To push "Start "

Now, The LED display will show “Firmware Update ,Please Wait” .The old firmware will be automatically deleted, and then the new firmware will be loaded.

The upgrade time is about 70 seconds.

The flatbed cutter will restart automatically, upgraded successfully.

After the upgrade ,check the machine version number（click **settings** - **SystemInformation** – **FWVer**）, it should be “FW1.00.03”